**Technical assignment**

The following criteria are required for the frame and lid:

1. Different inscriptions must be provided so that water supply and sewerage network can be identified without opening the lid.

2. The year of manufacture must be marked on the frame cover

3. Must be made of cast iron GJS 400-15

4. European standard EN 124 class D400, for all types of vehicles for road and pedestrian use

5. The material to be supplied is used for A / M roads, therefore it must have a load capacity of 40 tons (confirmed by relevant documents, which must be submitted together with other documents and must meet Georgian and international standards and norms in this field.

6. Weight - at least 65 kg

7. The frame lid should have a shutter

8. The clamp ("stud") must be made of steel

9. The frame lid should have rubber



