**ნარჩენების შემგროვებელი მანქანის და ნარჩენების ურნების შეძენა**

**დუშეთის მუნიციპალიტეტისთვის**

**Procurement of waste collection truck and waste containers for Dusheti Municipaliy**

Caritas Czech Republic in Georgia is announcing a **tender for the procurement of Waste Collection Truck and waste collection bins for collection and transportation of waste in Dusheti Municipality** within the framework of the Slovak Aid financial contribution to the project “Sustainable Development of the Area of Aragvi Protected Landscape and the Local Communities”.

Tender is announced for companies that are engaged in the supply of new equipment for Dusheti Municipality.

The brief information about the equipment and technical specifications is provided below:

**Waste collection truck**

The waste truck has to be equipped with a compress system.

Minimum technical requirements:

* Release date: 2019 and above new unused
* Motor type: Turbodiesel
* Motor power: min. 270 hp, from 5.8 cm³ to 6.5 cm3
* Number of cylinders: 6
* Fuel: Diesel
* Range: Less than 5000 km
* Emission EU standards: No less than EURO 3
* Transmission: Manual
* Steering wheel side: left
* Hydraulic power steering: applicable
* Wheel formula/driving wheels: 4X2/Rear
* Breaking system: ABS EBL Disc Type
* Allowable absolute load: 18000 kg
* Capacity of fuel tank: No less than 200 litres
* Cargo capacity: No less than 12000 kg
* Seating capacity: No less than 1+2 including driver
* Number of wheels: 6+1
* Wheel size: No less than 295/80 R22.5
* Wheel base: 4185 mm
* Cabin width: No less than 2495 mm
* Cabin temperature control system: applicable

Additional equipment: 14+1,5 m3 capacity EN 1501

* Deflections for both backsides
* Yellow emergency lights
* Lights for night works
* Mud flaps for backside wheel
* Hydraulic hoist
* Nut for wheels
* Spare parts and exploitation manual in English
* Mirrors, including mirror for front bumper and panoramic side mirrors on both side of vehicle
* Sun visor on drivers’ side
* Emergency signal during backstroke
* Front and back tow bars

Refuse compressor requirements:

* Type: backside loading
* Platforms on both sides for labours
* Compress rate: 3:1
* Compatibility with containers: capacity of 120, 240, 660, 1100 litres according to EU standards

Materials: No less than 3mm stainless steel sheets, steel mark no less than HARDOX 450.

**The waste collection truck should have minimum 1-year warranty.**

**Waste containers**

* 1100l Metal hot galvanized bins with round lids
* Quantity: 14 units
* Lift arms and cover link 2.50 mm.
* Cover handles 3.00 mm.d.
* Carrier 4 pieces 360 degrees 200x50 mm. with large tongs in size, 2 of them with brakes and fork plates of 4.00 mm.
* Should be galvanized in **accordance** with the **TS EN ISO 1461** standard, with the Hot Dip Galvanizing system
* Must have **TS EN 840-3** Standard Conformity Certificate, with ± 5% tolerance

**To participate in the tender**

Interested and qualified companies should submit their bids in one PDF file to:

[**ccrg-tender@caritas.cz**](mailto:ccrg-tender@caritas.cz) no later than August 25, 2020 at 18:00.

**Bids should include the following information:**

• Name, address, contact person and phone number of the company;

• Evidence of relevant work experience;

• Copy of a registration certificate of the company;

• Price breakdown in Euro (should be provided including VAT);

• Time required for service delivery;

• Warranty terms and conditions.

Incomplete documentation will not be considered.

**Bids will be evaluated according to the following criteria:**

• Lower Price of the equipment;

• Warranty terms and conditions;

• Time required for the supply of the equipment.