**Requirements for foodcourt container.**

* The upper and lower parts should be covered with stainless steel sheets (min 0.5mm thick), which is shown in silver.
* The inside bottom and sides (on 10cm height) must be covered with stainless steel sheets (min 0.5mm thick) and connections should be sealed properly, to provide a waterproofing.
* Material: "Copiti" color laminated DSP is acceptable, or MDF with "Copiti" veneer, with appropriate varnish coating from the inside and outside. Stainless steel does not need varnish. Cronka-plastic, 1 mm thick. silver color.
* The top door should be horizontally hinged, with a free inner opening (gravitational). It should be kept in a strictly vertical position (with no tilt, either inside or outside).
* Bottom door - should be taken a) left side – 5 units and b) 6 units-right side, with ordinary hinges, vertically. With a lock-magnet button. no handles.
* Back side material and color is same as sides.
* No screws, or screw covers should be from outside.
* All panels connections previously must be properly sealed with silicone before assembling.
* The quantity – 11 units.

560

1140

**Gravity door**

550

60

100

290

710