**Black Sea Terminal LLC is announcing tender on removal of the sunken ship in Kulevi Port waters**

**Initial information:** theship sank in approximately ~400m distance from the Kulevi Port in 5-10 depths. The total retrievable weight of the wreck is estimated approximately 400-450 tons.

**Condition of Vessel Wreck**

Half- submerged in SEABED

Year of Sinking: 2008

Location: approximately ~400m from the port

Left wreck: 15-25% from total GRT of the vessel

**Please find some requirements below. For further details contact to the terminal**

**Method of removal:** As per method statement provided by the contractor based on underwater inspection.

**Scope of work:**

Removal of complete wreck, including pieces on seabed and fully submerged in seabed to the full satisfaction of the customer as per method statement provided by the contractor.

Remove and transport all wreck mentioned above to the designated place as identified by Customer at risk and cost of the Contractor.

Cleaning of the place from small parts and remaining of the ship.

**Equipment and Machinery:** To be provided by the contractor. To be certified in compliance with technical requirements.

**Qualification requirements:** All personnel involved in wreck removal operations must be certified and qualified for wreck removal operations.

**Other requirements:**

Contractor shall develop a project for the execution of works with an accurate description of all stages of work

Works shall be performed in compliance with the project agreed with the Customer and Maritime Transport Agency of Georgia

Works shall be performed in compliance with Health, Safety and Environmental requirements, as well as legal and other requirements.