 Server minimum requirements:

2x Core server (Rack mountable):

1.      Intel Xeon Processors each minimum 3.6 GHz (Platinum or Gold). Max 32 core with possibility of Socket expansion.

2.      Minimum DDR4 1 TB of Ram

3.      Local 2 SSD drive.

2x Infrastructure Blade system with 4 Servers.

1.      Blade system with SAN and LAN (10Gb) connectivity.

2.      Intel Xeon Processors each minimum 3.6 GHz (Platinum or Gold).

3.      Minimum DDR4 1 TB of Ram

4.      Local 2 SSD drive

 System must include vendor Hardware & Software support for 3 years.

Company Qualification Requirements:

 Proposed equipment must be new (unused) & factory packaged;

 MAF (Manufacturer Authorization Form) must be provided;

 Local Service Center (or Provider) must be referenced with official Letter

 Company must have minimum 1 certified engineer under proposed hardware and corresponded certificate must be provided;

 Company’s experience in local market must be min. 3 years;

 Company must be local partner of the provided hardware vendor;

 Hardware installation with deadlines must be considered in offer.

 Additionally installation should be depicted in detailed steps, with time schedule and personnel with certification;